@routing @bicycle @ferry
Feature: Bike - Handle ferry routes

    Background:
        Given the profile "bicycle"

    Scenario: Bike - Ferry route
        Given the node map
            """
            a b c
                d
                e f g
            """

        And the ways
            | nodes | highway | route | bicycle |
            | abc   | primary |       |         |
            | cde   |         | ferry | yes     |
            | efg   | primary |       |         |

        When I route I should get
            | from | to | route           |
            | a    | g  | abc,cde,efg,efg |
            | b    | f  | abc,cde,efg,efg |
            | e    | c  | cde,cde         |
            | e    | b  | cde,abc,abc     |
            | e    | a  | cde,abc,abc     |
            | c    | e  | cde,cde         |
            | c    | f  | cde,efg,efg     |
            | c    | g  | cde,efg,efg     |

    Scenario: Bike - Ferry duration, single node
        Given the node map
            """
            a b c d
                e f
                g h
                i j
            """

        And the ways
            | nodes | highway | route | bicycle | duration |
            | ab    | primary |       |         |          |
            | cd    | primary |       |         |          |
            | ef    | primary |       |         |          |
            | gh    | primary |       |         |          |
            | ij    | primary |       |         |          |
            | bc    |         | ferry | yes     | 0:01     |
            | be    |         | ferry | yes     | 0:10     |
            | bg    |         | ferry | yes     | 1:00     |
            | bi    |         | ferry | yes     | 10:00    |

    Scenario: Bike - Ferry duration, multiple nodes
        Given the node map
            """
            x         y
              a b c d
            """

        And the ways
            | nodes | highway | route | bicycle | duration |
            | xa    | primary |       |         |          |
            | yd    | primary |       |         |          |
            | abcd  |         | ferry | yes     | 1:00     |

        When I route I should get
            | from | to | route | time       |
            | a    | d  | abcd,abcd  | 3600s +-10 |
            | d    | a  | abcd,abcd  | 3600s +-10 |
